NXOpen.UF.Sf.ContactMeshData Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Sf.ContactMeshData Structure

NXOpen.UF.Sf.ContactMeshData is an alias for NXOpen.UF.SfContactMeshData_Struct

class `NXOpen.UF.``SfContactMeshData_Struct`

  Bases: `object`

  Refer to UF_SF_contact_mesh_data_s for documentation.

Fields

`NXOpen.UF.SfContactMeshData_Struct.ElementName` | refer to uf_sf_lang_names.h
`NXOpen.UF.SfContactMeshData_Struct.ElementDescritorTag` | Set it to NULL_TAG
`NXOpen.UF.SfContactMeshData_Struct.AlignTargetEdgeNode` | 0 - Equal Distance 1 - Minimum Distance or Normal To
`NXOpen.UF.SfContactMeshData_Struct.TargetEdgeNodeAlignMethod` | 0 - Minimum Distance 1 - Normal To
`NXOpen.UF.SfContactMeshData_Struct.NumberOfElms` | required
`NXOpen.UF.SfContactMeshData_Struct.GapTolOption` | 0 - Do not apply tol 1 - Apply gap tolerance
`NXOpen.UF.SfContactMeshData_Struct.GapTolerance` | Gap tolerance option 0: Don’t apply tolerance 1: Apply tolerance
`NXOpen.UF.SfContactMeshData_Struct.ContactEdge` | Tag of the contact edge.
`NXOpen.UF.SfContactMeshData_Struct.ContactEdgeMeshDir` | Direction of the mesh for the contact edge: UF_SF_MG_MESHDIR_FROM_START UF_SF_MG_MESHDIR_FROM_END
`NXOpen.UF.SfContactMeshData_Struct.ContactEdgeStartLimit` | Limit of edge starting for the contact edge.
`NXOpen.UF.SfContactMeshData_Struct.ContactEdgeEndLimit` | Limit of edge ending for the contact edge.
`NXOpen.UF.SfContactMeshData_Struct.TargetEdge` | Tag of the target edge.
`NXOpen.UF.SfContactMeshData_Struct.TargetEdgeMeshDir` | Direction of the mesh for the target edge: UF_SF_MG_MESHDIR_FROM_START UF_SF_MG_MESHDIR_FROM_END
`NXOpen.UF.SfContactMeshData_Struct.TargetEdgeStartLimit` | set start limits to 0 and end limits to 1 to build contact mesh between entire length of the edges.
`NXOpen.UF.SfContactMeshData_Struct.TargetEdgeEndLimit` | Limit of edge ending for the target edge.