InspectionConstructedFeatureBuilderMethodEnumType Enumeration — NXOpen Python API Reference 12.0.0 documentation

# InspectionConstructedFeatureBuilderMethodEnumType Enumeration

NXOpen.CAM.InspectionConstructedFeatureBuilder.MethodEnumType is an alias for NXOpen.CAM.InspectionConstructedFeatureBuilderMethodEnumType

class `NXOpen.CAM.``InspectionConstructedFeatureBuilderMethodEnumType`

  Bases: `object`

  Construction Method

  Enum Members

  Enum Member | Enum Member Description
  --- | ---
  BestFit | Best Fit a feature to point reducible subfeatures
  Transform | Transform a copy of a feature from one PCS to another PCS
  Intersection | Intersects features to form a point plane or circle feature
  Minimum | Finds the maximum feature measurement point in a specified direction
  Maximum | Finds the minimum feature measurement point in a specified direction
  Projection | Projects a measurement point onto a measured or nominal feature
  MoveByFeature | Moves a copy of a point reducible feature in a direction associated with another feature
  MoveByVector | Moves a copy of a point reducible feature in a user specifiec direction
  PerpendicularTo | Creates a feature perpendicular to a feature and through another feature
  ParallelTo | Creates a feature parallel to a feature and through another feature
  Offset | Creates a plane or line offset by a nominal amount to each subfeature
  Middle | Creates a point, plane or line at the middle of two sub features
  ConeDiameter | Creates a circle at diameter of a cone
  ConeDistance | Creates a circle at distance along a cone
  Extract | Creates a feature by extract neasurements from other features

  `ValueOf`()

    Returns enum member equivalent to the value passed. Useful for bit operations of enum members.

    Signature `ValueOf(value)`

    Parameters: | value – Any integer value or bit operation result of enum members:type value: int:returns: Enum member equivalent to the value passed.
    Return type: | Enum Member type.

    New in version NX9.0.1.

    License requirements: None.