NXOpen.UF.Modl.SnipsrfFeatureData Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Modl.SnipsrfFeatureData Structure

NXOpen.UF.Modl.SnipsrfFeatureData is an alias for NXOpen.UF.ModlSnipsrfFeatureData_Struct

class `NXOpen.UF.``ModlSnipsrfFeatureData_Struct`

  Bases: `object`

  Refer to UF_MODL_snipsrf_feature_data_s for documentation.

Fields

`NXOpen.UF.ModlSnipsrfFeatureData_Struct.EditFace` | NX eid of a face to be snipped
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.BoundaryType` | Snipping bounding object type
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.SnipCvString` | Profile defining the snip curve
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.SnippingPlane` | NX eid of plane used as snipping object, Used only if boundary_type is, UF_MODL_snipsurf_boundary_type_plane
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.ProjectVector` | Projection vector, Necessary only if boundary_type is, UF_MODL_snipsurf_boundary_type_curves
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.SnipOrDivide` | Flag indicating snipping or divide operation, 0: Divide, otherwise Snipping operation Does not play any role during snip surface feature editing
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.RegionPointUv` | Region point on the edit_face indicating the retained side of the face divided by imprinted snipping curve.
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.ProjectMethod` | Project methods:0- along surface normal, 1- along view direction, 2- along x direction, 3- along y direction, 4- along z direction, 5- along given vector
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.RefitMethod` | Surface refitting method
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.RefitDegree` | Refit direction degree, Necessary if refit_type is, UF_MODL_snipsurf_refit_method_deg_patch or UF_MODL_snipsurf_refit_method_deg_tol
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.RefitPatches` | Refit direction patches, Necessary if refit_type is, UF_MODL_snipsurf_refit_method_deg_patch or UF_MODL_snipsurf_refit_method_patch_tol
`NXOpen.UF.ModlSnipsrfFeatureData_Struct.Tols` | Tolerance used for refitting, Necessary if refit_type is, UF_MODL_snipsurf_refit_method_deg_tol or UF_MODL_snipsurf_refit_method_patch_tol