MechanicalRoutingSubsetBuilderSurroundingDataRecipeMethod Enumeration — NXOpen Python API Reference 12.0.0 documentation

# MechanicalRoutingSubsetBuilderSurroundingDataRecipeMethod Enumeration

NXOpen.Assemblies.MechanicalRoutingSubsetBuilder.SurroundingDataRecipeMethod is an alias for NXOpen.Assemblies.MechanicalRoutingSubsetBuilderSurroundingDataRecipeMethod

class `NXOpen.Assemblies.``MechanicalRoutingSubsetBuilderSurroundingDataRecipeMethod`

  Bases: `object`

  Represents the method to use to determine the surrounding data corresponding to the routing design content that has been loaded. 1. None : No surrounding data to be loaded. 2. ProximityRoutingContent : This means surrounding data for the runs, this is related to the DE’s that are in proximity to the DEs constituting the run. 3. Manual: An empty Surrounding Object Subset will be created

  Enum Members

  Enum Member | Enum Member Description
  --- | ---

  NotSet

  ProximitytoRoutingContent

  Manual

  `ValueOf`()

    Returns enum member equivalent to the value passed. Useful for bit operations of enum members.

    Signature `ValueOf(value)`

    Parameters: | value – Any integer value or bit operation result of enum members:type value: int:returns: Enum member equivalent to the value passed.
    Return type: | Enum Member type.

    New in version NX9.0.1.

    License requirements: None.