NXOpen.UF.Sf.MidsrfUserParms Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Sf.MidsrfUserParms Structure

NXOpen.UF.Sf.MidsrfUserParms is an alias for NXOpen.UF.SfMidsrfUserParms_Struct

class `NXOpen.UF.``SfMidsrfUserParms_Struct`

  Bases: `object`

  Refer to UF_SF_midsrf_user_parms_s for documentation.

Fields

`NXOpen.UF.SfMidsrfUserParms_Struct.SolidBody` | Tag of the target solid body.
`NXOpen.UF.SfMidsrfUserParms_Struct.NumSheetBodies` | Number of sheet bodies.
`NXOpen.UF.SfMidsrfUserParms_Struct.SheetBodiesA` | Array of sheet body tags that will define the midsurface of the selected target solid body.
`NXOpen.UF.SfMidsrfUserParms_Struct.Thickness` | Thickness value to be used at formatting time whenever the automatic thickness extraction fails.
`NXOpen.UF.SfMidsrfUserParms_Struct.ConstThickness` | Constant thickness of all nodes of the midsurface.