NXOpen.UF.Curve.Bcmmcp Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Curve.Bcmmcp Structure

NXOpen.UF.Curve.Bcmmcp is an alias for NXOpen.UF.CurveBcmmcp_Struct

class `NXOpen.UF.``CurveBcmmcp_Struct`

  Bases: `object`

  Refer to UF_CURVE_BCMMCP_s for documentation.

Fields

`NXOpen.UF.CurveBcmmcp_Struct.LimPar1` | limit of start segment (SS)
`NXOpen.UF.CurveBcmmcp_Struct.LimPar2` | limit of end segment (ES)
`NXOpen.UF.CurveBcmmcp_Struct.DispPar1` | left limit of inner segment
`NXOpen.UF.CurveBcmmcp_Struct.DispPar2` | right limit of inner segment
`NXOpen.UF.CurveBcmmcp_Struct.Distance1` | distance to move e1 needed depending on selected displace_method
`NXOpen.UF.CurveBcmmcp_Struct.Distance2` | distance to move e2 needed depending on selected displace_method
`NXOpen.UF.CurveBcmmcp_Struct.Vector1` | direction to move e1 needed depending on selected displace_method
`NXOpen.UF.CurveBcmmcp_Struct.Vector2` | direction to move e2 needed depending on selected displace_method
`NXOpen.UF.CurveBcmmcp_Struct.DirPt1` | new location for e1 needed depending on selected displace_method
`NXOpen.UF.CurveBcmmcp_Struct.DirPt2` | new location for e2 needed depending on selected displace_method
`NXOpen.UF.CurveBcmmcp_Struct.DisplaceMethod1` | displacement method for e1
`NXOpen.UF.CurveBcmmcp_Struct.DisplaceMethod2` | displacement method for e2