TurnCutterClearance Class — NXOpen Python API Reference 12.0.0 documentation

# TurnCutterClearance Class

class `NXOpen.CAM.``TurnCutterClearance`

  Bases: `NXOpen.TaggedObject`

  Represents a `NXOpen.CAM.TurnCutterClearance`

  New in version NX6.0.0.

# Properties

Property | Description
--- | ---
FirstCuttingEdge | Returns or sets the first cutting edge clearance angle
LastCuttingEdge | Returns or sets the last cutting edge clearance angle
Tag | Returns the Tag for this object.

# Methods

# Property Detail

## FirstCuttingEdge

`TurnCutterClearance.``FirstCuttingEdge`

  Returns or sets the first cutting edge clearance angle

  `-------------------------------------`

  Getter Method

  Signature `FirstCuttingEdge`

  Returns: | the first cutting edge clearance angle
  Return type: | float

  New in version NX6.0.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `FirstCuttingEdge`

  Parameters: | newValue (float) – the first cutting edge clearance angle

  New in version NX6.0.0.

  License requirements: cam_base (“CAM BASE”)

## LastCuttingEdge

`TurnCutterClearance.``LastCuttingEdge`

  Returns or sets the last cutting edge clearance angle

  `-------------------------------------`

  Getter Method

  Signature `LastCuttingEdge`

  Returns: | the last cutting edge clearance angle
  Return type: | float

  New in version NX6.0.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `LastCuttingEdge`

  Parameters: | newValue (float) – the last cutting edge clearance angle

  New in version NX6.0.0.

  License requirements: cam_base (“CAM BASE”)