ResultMeasureResultAllOptions Class — NXOpen Python API Reference 12.0.0 documentation

# ResultMeasureResultAllOptions Class

class `NXOpen.CAE.``ResultMeasureResultAllOptions`

  Bases: `NXOpen.CAE.ResultMeasureResultOptions`

  Represents the combination of all result options for result measure

  To obtain an instance of this class use `NXOpen.CAE.ResultMeasureCollection`.

  New in version NX8.5.0.

# Methods

Method | Description
--- | ---
Dispose | Frees the object from memory.
SetAbsoluteValue | Set the option to use absolute values
SetAddBeamFillets | Set the option to add beam fillets for calculation of beam stresses only
SetBeamFilletRadius | Set the beam fillet radius if adding beam fillets for calculation of beam results only
SetBeamSection | Set the beam section for beam stress/strain results
SetCalculateBeamResults | Set the option to calculate beam stresses for beam results only
SetCoordinateSystem | Set the coordinate system for directional components
SetOperation | Set the operation type
SetPlynum | Set the ply num in result option
SetShellSection | Set the shell section for shell stress/strain results
SetUnit | Set the unit

# Method Detail

## Dispose

`ResultMeasureResultAllOptions.``Dispose`

  Frees the object from memory.

  After this method is called, it is illegal to use the object. In .NET, this method is automatically called when the object is deleted by the garbage collector.

  Signature `Dispose()`

  New in version NX8.5.0.

  License requirements: None.

## SetAddBeamFillets

`ResultMeasureResultAllOptions.``SetAddBeamFillets`

  Set the option to add beam fillets for calculation of beam stresses only

  Signature `SetAddBeamFillets(bAddBeamFillets)`

  Parameters: | bAddBeamFillets (bool) –

  New in version NX8.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”)

## SetBeamFilletRadius

`ResultMeasureResultAllOptions.``SetBeamFilletRadius`

  Set the beam fillet radius if adding beam fillets for calculation of beam results only

  Signature `SetBeamFilletRadius(beamFilletRadius)`

  Parameters: | beamFilletRadius (float) –

  New in version NX8.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”)

## SetBeamSection

`ResultMeasureResultAllOptions.``SetBeamSection`

  Set the beam section for beam stress/strain results

  Signature `SetBeamSection(eBeamSect)`

  Parameters: | eBeamSect (`NXOpen.CAE.ResultSection`) –

  New in version NX8.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”)

## SetCalculateBeamResults

`ResultMeasureResultAllOptions.``SetCalculateBeamResults`

  Set the option to calculate beam stresses for beam results only

  Signature `SetCalculateBeamResults(bCalcBeamResults)`

  Parameters: | bCalcBeamResults (bool) –

  New in version NX8.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”)

## SetCoordinateSystem

`ResultMeasureResultAllOptions.``SetCoordinateSystem`

  Set the coordinate system for directional components

  Signature `SetCoordinateSystem(eCsys)`

  Parameters: | eCsys (`NXOpen.CAE.ResultCoordinateSystem`) –

  New in version NX8.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”)

## SetShellSection

`ResultMeasureResultAllOptions.``SetShellSection`

  Set the shell section for shell stress/strain results

  Signature `SetShellSection(eShellSect)`

  Parameters: | eShellSect (`NXOpen.CAE.ResultSection`) –

  New in version NX8.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”)