ResultParameters Class — NXOpen Python API Reference 12.0.0 documentation

# ResultParameters Class

class `NXOpen.CAE.``ResultParameters`

  Bases: `NXOpen.TaggedObject`

  This class is worked as a packet of information that can be either be used to change result state or pass around for information exchange between two `NXOpen.CAE.ResultAccess` objects.

  <br/>Use `NXOpen.CAE.ResultManager` to create an `NXOpen.CAE.ResultParameters`

  <br/>You can modifiy these values but validation of correctness will only be perfomed when this object is set to a `NXOpen.CAE.ResultAccess` object

  To obtain an instance of this class use `NXOpen.Session.ResultManager()`.

  New in version NX6.0.2.

# Properties

Property | Description
--- | ---
Tag | Returns the Tag for this object.

# Methods

Method | Description
--- | ---
AskSectionPlyLayer | Ask section, ply and layer
DisplayMidnodeValue | This is display only command.
GetAbsoluteValue | Ask whether all values are absolute values
GetAveragingCriteria | Ask averaging criteria.
GetAxiSymmetricParameters | Get Axi Symmetric Parameters type
GetBeamFilletRadius | Return the fillet radius
GetBeamFillets | Return the fillets flag
GetBeamResultsInLocalCoordinateSystem | Identifies whether beam results are presented in local coordinate system (if true) or in the same coordinate system as the rest of the model
GetCalculateBeamStrResults | Ask if beam stresses and strains are calculated from element forces and section geometry
GetComplexCriterion | If result is complex it returns which component is set(like real or imaginary)
GetComputationType | Get computing type.
GetComputeOnVisible | Ask whether elements which are not visible are to be considerd for Averaging, Summing, Gap/Discontinuity calculations
GetConvertedDBref | Ask the converted DB Reference value
GetCoordinateSystem | Ask result coordinate system
GetCyclicSymmetricParameters | Get Cyclic Symmetric Parameters type
GetDBScaling | Ask whether dB Scaling is on or not
GetDBreference | Ask the dB Reference value
GetDBscale | Ask the dB Scale value
GetDbSettings | Gets the dBSettings object required for dB Scaling
GetDiscontinuityMethod | Ask discontinuity method
GetElementValueCriterion | Ask how element the result is defined.
GetExcludeElementsNotVisible | Ask whether elements which are not visible are consider for summation
GetGenericResultType | Ask Result type
GetIsReferenceNode | Ask if the reference node will be used for result
GetIteration | Ask Current iteration number This method has been deprecated.
GetLoadcase | Ask Current loadcase number This method has been deprecated.
GetPhaseAngle | Ask phase angle.
GetReferenceNodeLabel | Returns the node label which identifies the reference node used when plotting the result
GetResultBeamSection | Ask section where beam results are defined
GetResultComponent | Ask result component
GetResultDataLocation | Ask FE entity where the result is defined This method has been deprecated.
GetResultDataQuantity | Ask result type This method has been deprecated.
GetResultDataSection | Ask section of a FE entity where the result is defined This method has been deprecated.
GetResultShellSection | Ask section where shell results are defined
GetResultType | Ask Result type This method has been deprecated.
GetRotationAxisOfAbsoluteCyndricalCSYS | Get axis of rotation for axisyymettric results
GetScale | Ask scale
GetSelectedCoordinateSystem | Ask selected coordinate system in which results are to be presented
GetTensorComponentAbsoluteValue | Get the method used when calculating the absolute values for the derived components of `CAE.ResultDataType.Tensor` like `CAE.ResultComponent.MaximumPrincipal`
GetUnit | Ask result unit
InitAveragingCriteria | Ask default averaging criteria
IsForcedElementResult | Ask whether the result is converted as element result
IsMidnodeValueDisplayed | Ask whether the result at mid nodes are ignored
MakeElementResult | Make Nodal and Element-Nodal result to Element Result.
SetAbsoluteValue | Set all values to absolute values.
SetAveragingCriteria | Set averaging criteria
SetAxiSymmetricParameters | Set Axi Symmetric Parameters type
SetBeamFilletRadius | Sets the fillet radius as a fraction of the adjacent dimensions
SetBeamFillets | Sets the fillets flag
SetBeamResultsInLocalCoordinateSystem | Presents beam results in local coordinate system (if flag is true) or in the same coordinate system as the rest of the model
SetCalculateBeamStrResults | Sets a flag to calculate beam stresses and strains from element forces and section geometry (if available).
SetComplexCriterion | Set complex criteria
SetComputationType | Set computing type.
SetComputeOnVisible | Exclude or include elements which are not visible for Averaging, Summing, Gap/Discontinuity calculations
SetCoordinateSystem | Set result coordinate system
SetCyclicSymmetricParameters | Set Cyclic Symmetric Parameters type
SetDBReference | Set the dB Reference value
SetDBScaling | Set the dB Scaling on or off
SetDBscale | Set the dB Scale value
SetDiscontinuityMethod | Set discontinuity method
SetElementValueCriterion | Set how element the result is defined This option is only valid for nodal and elemen-nodal result; dose not do anything for element result.
SetExcludeElementsNotVisible | Exclude or include elements which are not visible for computing with sum option.
SetGenericResultType | Set Result type
SetIsReferenceNode | Sets the flag if the reference node will be used for result
SetLoadcaseIteration | Set Current loadcase and iteration.
SetPhaseAngle | Sets the phase angle at which result will be evaluated.
SetReferenceNodeLabel | Sets the node label which identifies the reference node used when plotting the result
SetResultBeamSection | Set section where beam results are defined
SetResultComponent | Set result component
SetResultDataLocation | Set FE entity where the result is defined This method has been deprecated.
SetResultDataQuantity | Set result quantity This method has been deprecated.
SetResultDataSection | Set section of a FE entity where the result is defined This method has been deprecated.
SetResultShellSection | Set section where shell results are defined
SetResultType | Set Result type This method has been deprecated.
SetRotationAxisOfAbsoluteCyndricalCSYS | Set axis of rotation for axisymmetric results
SetScale | Set scale.
SetSectionPlyLayer | Set section, ply and layer
SetSelectedCoordinateSystem | Set selected coordinate system in which results are to be presented Coordinate systems labels defined in a result file can be retrieved using `CAE.Result.GetResultCoordinateSystems()`
SetTensorComponentAbsoluteValue | Set the method used when calculating the absolute values for the derived components of `CAE.ResultDataType.Tensor` like `CAE.ResultComponent.MaximumPrincipal`
SetUnit | Set result unit

# Method Detail

## AskSectionPlyLayer

`ResultParameters.``AskSectionPlyLayer`

  Ask section, ply and layer

  Signature `AskSectionPlyLayer()`

  Returns: | a tuple
  Return type: | A tuple consisting of (layer, section, ply) layer is a int. section is a int. ply is a int.

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## DisplayMidnodeValue

`ResultParameters.``DisplayMidnodeValue`

  This is display only command.

  Setting this value will not change modify ResultAccess queries. But Post view will ignore midnode values during display

  Signature `DisplayMidnodeValue(display)`

  Parameters: | display (bool) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetAbsoluteValue

`ResultParameters.``GetAbsoluteValue`

  Ask whether all values are absolute values

  Signature `GetAbsoluteValue()`

  Returns: |
  Return type: | bool

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetAveragingCriteria

`ResultParameters.``GetAveragingCriteria`

  Ask averaging criteria.

  Signature `GetAveragingCriteria()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultAveraging_Struct`

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetAxiSymmetricParameters

`ResultParameters.``GetAxiSymmetricParameters`

  Get Axi Symmetric Parameters type

  Signature `GetAxiSymmetricParameters()`

  Returns: |
  Return type: | `NXOpen.CAE.AxiSymmetricParameters`

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetBeamFilletRadius

`ResultParameters.``GetBeamFilletRadius`

  Return the fillet radius

  Signature `GetBeamFilletRadius()`

  Returns: |
  Return type: | float

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetBeamFillets

`ResultParameters.``GetBeamFillets`

  Return the fillets flag

  Signature `GetBeamFillets()`

  Returns: |
  Return type: | bool

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetBeamResultsInLocalCoordinateSystem

`ResultParameters.``GetBeamResultsInLocalCoordinateSystem`

  Identifies whether beam results are presented in local coordinate system (if true) or in the same coordinate system as the rest of the model

  Signature `GetBeamResultsInLocalCoordinateSystem()`

  Returns: |
  Return type: | bool

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetCalculateBeamStrResults

`ResultParameters.``GetCalculateBeamStrResults`

  Ask if beam stresses and strains are calculated from element forces and section geometry

  Signature `GetCalculateBeamStrResults()`

  Returns: |
  Return type: | bool

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetComplexCriterion

`ResultParameters.``GetComplexCriterion`

  If result is complex it returns which component is set(like real or imaginary)

  Signature `GetComplexCriterion()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultComplex`

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetComputationType

`ResultParameters.``GetComputationType`

  Get computing type.

  Signature `GetComputationType()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultComputationType`

  New in version NX7.5.1.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetComputeOnVisible

`ResultParameters.``GetComputeOnVisible`

  Ask whether elements which are not visible are to be considerd for Averaging, Summing, Gap/Discontinuity calculations

  Signature `GetComputeOnVisible()`

  Returns: |
  Return type: | bool

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetConvertedDBref

`ResultParameters.``GetConvertedDBref`

  Ask the converted DB Reference value

  Signature `GetConvertedDBref()`

  Returns: |
  Return type: | float

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetCoordinateSystem

`ResultParameters.``GetCoordinateSystem`

  Ask result coordinate system

  Signature `GetCoordinateSystem()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultCoordinateSystem`

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetCyclicSymmetricParameters

`ResultParameters.``GetCyclicSymmetricParameters`

  Get Cyclic Symmetric Parameters type

  Signature `GetCyclicSymmetricParameters()`

  Returns: |
  Return type: | `NXOpen.CAE.CyclicSymmetricParameters`

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetDBScaling

`ResultParameters.``GetDBScaling`

  Ask whether dB Scaling is on or not

  Signature `GetDBScaling()`

  Returns: |
  Return type: | bool

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetDBreference

`ResultParameters.``GetDBreference`

  Ask the dB Reference value

  Signature `GetDBreference()`

  Returns: |
  Return type: | float

  New in version NX11.0.0.

  Deprecated since version NX12.0.0: Use `NXOpen.CAE.ResultParameters.GetDbSettings()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetDBscale

`ResultParameters.``GetDBscale`

  Ask the dB Scale value

  Signature `GetDBscale()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultDbScale`

  New in version NX11.0.0.

  Deprecated since version NX12.0.0: Use `NXOpen.CAE.ResultParameters.GetDbSettings()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetDbSettings

`ResultParameters.``GetDbSettings`

  Gets the dBSettings object required for dB Scaling

  Signature `GetDbSettings()`

  Returns: |
  Return type: | `NXOpen.CAE.SignalProcessingDBSettings`

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetDiscontinuityMethod

`ResultParameters.``GetDiscontinuityMethod`

  Ask discontinuity method

  Signature `GetDiscontinuityMethod()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultDiscontinuityMethod`

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”)

## GetElementValueCriterion

`ResultParameters.``GetElementValueCriterion`

  Ask how element the result is defined.

  This option is only valid for nodal and elemen-nodal result.

  Signature `GetElementValueCriterion()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultElementValueCriterion`

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetExcludeElementsNotVisible

`ResultParameters.``GetExcludeElementsNotVisible`

  Ask whether elements which are not visible are consider for summation

  Signature `GetExcludeElementsNotVisible()`

  Returns: |
  Return type: | bool

  New in version NX7.5.1.

  Deprecated since version NX12.0.0: Use `NXOpen.CAE.ResultParameters.GetComputeOnVisible()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetGenericResultType

`ResultParameters.``GetGenericResultType`

  Ask Result type

  Signature `GetGenericResultType()`

  Returns: |
  Return type: | `NXOpen.CAE.BaseResultType`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetIsReferenceNode

`ResultParameters.``GetIsReferenceNode`

  Ask if the reference node will be used for result

  Signature `GetIsReferenceNode()`

  Returns: |
  Return type: | bool

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetIteration

`ResultParameters.``GetIteration`

  Ask Current iteration number This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `GetIteration()`

  Returns: |
  Return type: | int

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetLoadcase

`ResultParameters.``GetLoadcase`

  Ask Current loadcase number This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `GetLoadcase()`

  Returns: |
  Return type: | int

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetPhaseAngle

`ResultParameters.``GetPhaseAngle`

  Ask phase angle.

  If complex result is set to Phaseangle type then user can specify an angle at which result will be evaluated

  Signature `GetPhaseAngle()`

  Returns: |
  Return type: | float

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetReferenceNodeLabel

`ResultParameters.``GetReferenceNodeLabel`

  Returns the node label which identifies the reference node used when plotting the result

  Signature `GetReferenceNodeLabel()`

  Returns: |
  Return type: | int

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetResultBeamSection

`ResultParameters.``GetResultBeamSection`

  Ask section where beam results are defined

  Signature `GetResultBeamSection()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultSection`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetResultComponent

`ResultParameters.``GetResultComponent`

  Ask result component

  Signature `GetResultComponent()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultComponent`

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetResultDataLocation

`ResultParameters.``GetResultDataLocation`

  Ask FE entity where the result is defined This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `GetResultDataLocation()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultLocation`

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.BaseResultType.Location()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetResultDataQuantity

`ResultParameters.``GetResultDataQuantity`

  Ask result type This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `GetResultDataQuantity()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultQuantity`

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetResultDataSection

`ResultParameters.``GetResultDataSection`

  Ask section of a FE entity where the result is defined This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `GetResultDataSection()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultSection`

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetResultShellSection

`ResultParameters.``GetResultShellSection`

  Ask section where shell results are defined

  Signature `GetResultShellSection()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultSection`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetResultType

`ResultParameters.``GetResultType`

  Ask Result type This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `GetResultType()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultType_Struct`

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetRotationAxisOfAbsoluteCyndricalCSYS

`ResultParameters.``GetRotationAxisOfAbsoluteCyndricalCSYS`

  Get axis of rotation for axisyymettric results

  Signature `GetRotationAxisOfAbsoluteCyndricalCSYS()`

  Returns: |
  Return type: | `NXOpen.CAE.PostAxisymetricAxis`

  New in version NX10.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetScale

`ResultParameters.``GetScale`

  Ask scale

  Signature `GetScale()`

  Returns: |
  Return type: | float

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetSelectedCoordinateSystem

`ResultParameters.``GetSelectedCoordinateSystem`

  Ask selected coordinate system in which results are to be presented

  Signature `GetSelectedCoordinateSystem()`

  Returns: | a tuple
  Return type: | A tuple consisting of (source, id). source is a `NXOpen.CAE.ResultCoordinateSystemSource`. id is a int.

  New in version NX7.5.1.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetTensorComponentAbsoluteValue

`ResultParameters.``GetTensorComponentAbsoluteValue`

  Get the method used when calculating the absolute values for the derived components of `CAE.ResultDataType.Tensor` like `CAE.ResultComponent.MaximumPrincipal`

  Signature `GetTensorComponentAbsoluteValue()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultTensorDerivedAbsolute`

  New in version NX8.0.1.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## GetUnit

`ResultParameters.``GetUnit`

  Ask result unit

  Signature `GetUnit()`

  Returns: |
  Return type: | `NXOpen.Unit`

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## InitAveragingCriteria

`ResultParameters.``InitAveragingCriteria`

  Ask default averaging criteria

  Signature `InitAveragingCriteria()`

  Returns: |
  Return type: | `NXOpen.CAE.ResultAveraging_Struct`

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## IsForcedElementResult

`ResultParameters.``IsForcedElementResult`

  Ask whether the result is converted as element result

  Signature `IsForcedElementResult()`

  Returns: |
  Return type: | bool

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## IsMidnodeValueDisplayed

`ResultParameters.``IsMidnodeValueDisplayed`

  Ask whether the result at mid nodes are ignored

  Signature `IsMidnodeValueDisplayed()`

  Returns: |
  Return type: | bool

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## MakeElementResult

`ResultParameters.``MakeElementResult`

  Make Nodal and Element-Nodal result to Element Result.

  Does not do anything if the result is element result already. To define what value should be used to represent an element, use `NXOpen.CAE.ResultParameters.SetElementValueCriterion()`

  Signature `MakeElementResult(elementResult)`

  Parameters: | elementResult (bool) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetAbsoluteValue

`ResultParameters.``SetAbsoluteValue`

  Set all values to absolute values.

  Warning: Once converted to absolute value it is not possible to revert to original values.

  Signature `SetAbsoluteValue(absolute)`

  Parameters: | absolute (bool) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetAveragingCriteria

`ResultParameters.``SetAveragingCriteria`

  Set averaging criteria

  Signature `SetAveragingCriteria(average)`

  Parameters: | average (`NXOpen.CAE.ResultAveraging_Struct`) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetAxiSymmetricParameters

`ResultParameters.``SetAxiSymmetricParameters`

  Set Axi Symmetric Parameters type

  Signature `SetAxiSymmetricParameters(type)`

  Parameters: | type (`NXOpen.CAE.AxiSymmetricParameters`) –

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetBeamFilletRadius

`ResultParameters.``SetBeamFilletRadius`

  Sets the fillet radius as a fraction of the adjacent dimensions

  Signature `SetBeamFilletRadius(beamFilletRadius)`

  Parameters: | beamFilletRadius (float) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetBeamFillets

`ResultParameters.``SetBeamFillets`

  Sets the fillets flag

  Signature `SetBeamFillets(beamFillets)`

  Parameters: | beamFillets (bool) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetBeamResultsInLocalCoordinateSystem

`ResultParameters.``SetBeamResultsInLocalCoordinateSystem`

  Presents beam results in local coordinate system (if flag is true) or in the same coordinate system as the rest of the model

  Signature `SetBeamResultsInLocalCoordinateSystem(local)`

  Parameters: | local (bool) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetCalculateBeamStrResults

`ResultParameters.``SetCalculateBeamStrResults`

  Sets a flag to calculate beam stresses and strains from element forces and section geometry (if available).

  Does not affect other result types and element types

  Signature `SetCalculateBeamStrResults(calcBeamStrResults)`

  Parameters: | calcBeamStrResults (bool) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetComplexCriterion

`ResultParameters.``SetComplexCriterion`

  Set complex criteria

  Signature `SetComplexCriterion(complex)`

  Parameters: | complex (`NXOpen.CAE.ResultComplex`) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetComputationType

`ResultParameters.``SetComputationType`

  Set computing type.

  Signature `SetComputationType(computeType)`

  Parameters: | computeType (`NXOpen.CAE.ResultComputationType`) –

  New in version NX7.5.1.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetComputeOnVisible

`ResultParameters.``SetComputeOnVisible`

  Exclude or include elements which are not visible for Averaging, Summing, Gap/Discontinuity calculations

  Signature `SetComputeOnVisible(excludeElements)`

  Parameters: | excludeElements (bool) –

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetCoordinateSystem

`ResultParameters.``SetCoordinateSystem`

  Set result coordinate system

  Signature `SetCoordinateSystem(coordinate)`

  Parameters: | coordinate (`NXOpen.CAE.ResultCoordinateSystem`) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetCyclicSymmetricParameters

`ResultParameters.``SetCyclicSymmetricParameters`

  Set Cyclic Symmetric Parameters type

  Signature `SetCyclicSymmetricParameters(type)`

  Parameters: | type (`NXOpen.CAE.CyclicSymmetricParameters`) –

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetDBReference

`ResultParameters.``SetDBReference`

  Set the dB Reference value

  Signature `SetDBReference(dBreference)`

  Parameters: | dBreference (float) –

  New in version NX11.0.0.

  Deprecated since version NX12.0.0: Use `NXOpen.CAE.ResultParameters.GetDbSettings()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetDBScaling

`ResultParameters.``SetDBScaling`

  Set the dB Scaling on or off

  Signature `SetDBScaling(dBscaling)`

  Parameters: | dBscaling (int) –

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetDBscale

`ResultParameters.``SetDBscale`

  Set the dB Scale value

  Signature `SetDBscale(dbScale)`

  Parameters: | dbScale (`NXOpen.CAE.ResultDbScale`) –

  New in version NX11.0.0.

  Deprecated since version NX12.0.0: Use `NXOpen.CAE.ResultParameters.GetDbSettings()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetDiscontinuityMethod

`ResultParameters.``SetDiscontinuityMethod`

  Set discontinuity method

  Signature `SetDiscontinuityMethod(discontinuity)`

  Parameters: | discontinuity (`NXOpen.CAE.ResultDiscontinuityMethod`) –

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”)

## SetElementValueCriterion

`ResultParameters.``SetElementValueCriterion`

  Set how element the result is defined This option is only valid for nodal and elemen-nodal result; dose not do anything for element result.

  Signature `SetElementValueCriterion(criteria)`

  Parameters: | criteria (`NXOpen.CAE.ResultElementValueCriterion`) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetExcludeElementsNotVisible

`ResultParameters.``SetExcludeElementsNotVisible`

  Exclude or include elements which are not visible for computing with sum option.

  Signature `SetExcludeElementsNotVisible(excludeElements)`

  Parameters: | excludeElements (bool) –

  New in version NX7.5.1.

  Deprecated since version NX12.0.0: Use `NXOpen.CAE.ResultParameters.SetComputeOnVisible()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetGenericResultType

`ResultParameters.``SetGenericResultType`

  Set Result type

  Signature `SetGenericResultType(type)`

  Parameters: | type (`NXOpen.CAE.BaseResultType`) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetIsReferenceNode

`ResultParameters.``SetIsReferenceNode`

  Sets the flag if the reference node will be used for result

  Signature `SetIsReferenceNode(isReferenceNode)`

  Parameters: | isReferenceNode (bool) –

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetLoadcaseIteration

`ResultParameters.``SetLoadcaseIteration`

  Set Current loadcase and iteration.

  This method has been deprecated. This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `SetLoadcaseIteration(loadcase, iteration)`

  Parameters:

  - loadcase (int) – loadcase number varies from 0 to N-1
  - iteration (int) – iteration number varies from 0 to N-1

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.SetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetPhaseAngle

`ResultParameters.``SetPhaseAngle`

  Sets the phase angle at which result will be evaluated.

  This is only value if complex result is set to the PhaseAngle type

  Signature `SetPhaseAngle(angle)`

  Parameters: | angle (float) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetReferenceNodeLabel

`ResultParameters.``SetReferenceNodeLabel`

  Sets the node label which identifies the reference node used when plotting the result

  Signature `SetReferenceNodeLabel(referenceNodeLabel)`

  Parameters: | referenceNodeLabel (int) –

  New in version NX11.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetResultBeamSection

`ResultParameters.``SetResultBeamSection`

  Set section where beam results are defined

  Signature `SetResultBeamSection(section)`

  Parameters: | section (`NXOpen.CAE.ResultSection`) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetResultComponent

`ResultParameters.``SetResultComponent`

  Set result component

  Signature `SetResultComponent(component)`

  Parameters: | component (`NXOpen.CAE.ResultComponent`) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetResultDataLocation

`ResultParameters.``SetResultDataLocation`

  Set FE entity where the result is defined This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `SetResultDataLocation(location)`

  Parameters: | location (`NXOpen.CAE.ResultLocation`) –

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetResultDataQuantity

`ResultParameters.``SetResultDataQuantity`

  Set result quantity This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `SetResultDataQuantity(quantity)`

  Parameters: | quantity (`NXOpen.CAE.ResultQuantity`) –

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetResultDataSection

`ResultParameters.``SetResultDataSection`

  Set section of a FE entity where the result is defined This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `SetResultDataSection(section)`

  Parameters: | section (`NXOpen.CAE.ResultSection`) –

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetResultShellSection

`ResultParameters.``SetResultShellSection`

  Set section where shell results are defined

  Signature `SetResultShellSection(section)`

  Parameters: | section (`NXOpen.CAE.ResultSection`) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetResultType

`ResultParameters.``SetResultType`

  Set Result type This method has been deprecated.

  This functionality was moved to this class `NXOpen.CAE.BaseResultType`, which can be obtained by using `NXOpen.CAE.ResultParameters.GetGenericResultType()`.

  Signature `SetResultType(type)`

  Parameters: | type (`NXOpen.CAE.ResultType_Struct`) –

  New in version NX6.0.2.

  Deprecated since version NX8.0.0: Use `NXOpen.CAE.ResultParameters.GetGenericResultType()` instead.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetRotationAxisOfAbsoluteCyndricalCSYS

`ResultParameters.``SetRotationAxisOfAbsoluteCyndricalCSYS`

  Set axis of rotation for axisymmetric results

  Signature `SetRotationAxisOfAbsoluteCyndricalCSYS(axis)`

  Parameters: | axis (`NXOpen.CAE.PostAxisymetricAxis`) –

  New in version NX10.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetScale

`ResultParameters.``SetScale`

  Set scale.

  This will affect all subsequent result query.

  Signature `SetScale(scale)`

  Parameters: | scale (float) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetSectionPlyLayer

`ResultParameters.``SetSectionPlyLayer`

  Set section, ply and layer

  Signature `SetSectionPlyLayer(section, ply, layer)`

  Parameters:

  - section (int) –
  - ply (int) –
  - layer (int) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetSelectedCoordinateSystem

`ResultParameters.``SetSelectedCoordinateSystem`

  Set selected coordinate system in which results are to be presented Coordinate systems labels defined in a result file can be retrieved using `CAE.Result.GetResultCoordinateSystems()`

  Signature `SetSelectedCoordinateSystem(source, id)`

  Parameters:

  - source (`NXOpen.CAE.ResultCoordinateSystemSource`) –
  - id (int) –

  New in version NX7.5.1.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetTensorComponentAbsoluteValue

`ResultParameters.``SetTensorComponentAbsoluteValue`

  Set the method used when calculating the absolute values for the derived components of `CAE.ResultDataType.Tensor` like `CAE.ResultComponent.MaximumPrincipal`

  Signature `SetTensorComponentAbsoluteValue(absolute)`

  Parameters: | absolute (`NXOpen.CAE.ResultTensorDerivedAbsolute`) –

  New in version NX8.0.1.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)

## SetUnit

`ResultParameters.``SetUnit`

  Set result unit

  Signature `SetUnit(unit)`

  Parameters: | unit (`NXOpen.Unit`) –

  New in version NX6.0.2.

  License requirements: nx_masterfem (“Finite Element Modeling”) OR nx_design_sim (“NX Design Simulation”) OR sc_results_viewer (” Simcenter Results Viewer”)