AfuMathFastRMSInfo Class — NXOpen Python API Reference 12.0.0 documentation

# AfuMathFastRMSInfo Class

class `NXOpen.CAE.``AfuMathFastRMSInfo`

  Bases: `NXOpen.TransientObject`

  Represents the Fast RMS parameter information

  New in version NX11.0.0.

# Methods

Method | Description
--- | ---
Dispose | The object destructor
GetData | Get the Fast RMS Parameter Information
SetData | Set the Fast RMS Parameter Information

# Method Detail

## Dispose

`AfuMathFastRMSInfo.``Dispose`

  The object destructor

  Signature `Dispose()`

  New in version NX11.0.0.

  License requirements: None.

## GetData

`AfuMathFastRMSInfo.``GetData`

  Get the Fast RMS Parameter Information

  Signature `GetData()`

  Returns: | a tuple
  Return type: | A tuple consisting of (interpolationMethod, numberOfPoints, order, relativeOrder, useHighpassFilter, cutoffFraction, addSidelobes, slope) interpolationMethod is a int. the interpolation method numberOfPoints is a int. Get the Fast RMS PSD Fit number of points order is a int. the order relativeOrder is a int. the relative order useHighpassFilter is a int. the use highpass filter option cutoffFraction is a float. The filter frequency cutoff fraction addSidelobes is a int. the add sidelobes option slope is a float. the side lobes slope value

  New in version NX11.0.0.

  License requirements: None.

## SetData

`AfuMathFastRMSInfo.``SetData`

  Set the Fast RMS Parameter Information

  Signature `SetData(numberOfPoints, order, relativeOrder, useHighpassFilter, cutoffFraction, addSidelobes, slope, interpolationMethod)`

  Parameters:

  - numberOfPoints (int) – Set the Fast RMS PSD Fit number of points
  - order (int) – the order
  - relativeOrder (int) – the relative order
  - useHighpassFilter (int) – the use highpass filter option
  - cutoffFraction (float) – the filter frequency cutoff fraction
  - addSidelobes (int) – the add sidelobes option
  - slope (float) – the side lobes slope value
  - interpolationMethod (int) – the interpolation method

  New in version NX11.0.0.

  License requirements: None.