BreakCornerBuilder Class — NXOpen Python API Reference 12.0.0 documentation

# BreakCornerBuilder Class

class `NXOpen.Features.SheetMetal.``BreakCornerBuilder`

  Bases: `NXOpen.Features.SheetMetal.SheetmetalBaseBuilder`

  Represents a break corner feature builder.

  To create a new instance of this class, use `NXOpen.Features.SheetMetal.SheetmetalManager.CreateBreakCornerFeatureBuilder()`

  New in version NX4.0.0.

# Properties

Property | Description
--- | ---
ParentFeatureInternal | Returns or sets whether or not the latest timestamped parent feature of this feature should be made internal
PatchSolutionFlag | Returns or sets the patch solution flag
PatchSurfaceFilename | Returns or sets the patch surface filename
SurroundingPatchSurfaceFilename | Returns or sets the surrounding patch surface filename
Tag | Returns the Tag for this object.
Type | Returns or sets the type of the break corner.
Value | Returns the fillet radius or the setback value, depending on the type of the break corner.

# Methods

Method | Description
--- | ---
Commit | Commits any edits that have been applied to the builder.
CommitFeature | Commits the feature parameters and creates the feature
Destroy | Deletes the builder, and cleans up any objects created by the builder.
GetApplicationContext | Get the application context.
GetCommittedObjects | For builders that create more than one object, this method returns the objects that are created by commit.
GetEdges | The array of input edges for the break corner.
GetFaces | The array of input faces that implicitly include all connected sharp thickness edges as input for the break corner.
GetFeature | Returns the feature currently being edited by this builder.
GetObject | Returns the object currently being edited by this builder.
HideInternalParentFeatureAfterEdit | Re-suppress an internal parent feature (a slave feature) after it has been edited.
SetApplicationContext | Set the application context.
SetEdges | The array of input edges for the break corner.
SetFaces | The array of input faces that implicitly include all connected sharp thickness edges as input for the break corner.
SetParentFeatureInternal | Set the parent features which would be internal or slaves to the feature being created or commited
SetValue |
ShowInternalParentFeatureForEdit | Unsuppress an internal parent feature (a slave feature) so it can be edited.
ShowResults | Updates the model to reflect the result of an edit to the model for all builders that support showing results.
UnsetParentFeatureInternal | Set the internal parent feature of the feature being edited to external
Validate | Validate whether the inputs to the component are sufficient for commit to be called.
ValidateBuilderData | Verify that the builder data is valid for creating a break corner.

# Enumerations

BreakCornerBuilderTypeOptions Enumeration | This enum represents the break corner type.

# Property Detail

## Type

`BreakCornerBuilder.``Type`

  Returns or sets the type of the break corner.

  Specify `Features.SheetMetal.BreakCornerBuilderTypeOptions.Fillet` to fillet the edge. Specify `Features.SheetMetal.BreakCornerBuilderTypeOptions.ChamferEqualSetback` to chamfer the edge.

  `-------------------------------------`

  Getter Method

  Signature `Type`

  Returns: | Break corner type
  Return type: | `NXOpen.Features.SheetMetal.BreakCornerBuilderTypeOptions`

  New in version NX4.0.0.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)

  `-------------------------------------`

  Setter Method

  Signature `Type`

  Parameters: | type (`NXOpen.Features.SheetMetal.BreakCornerBuilderTypeOptions`) – Break corner type

  New in version NX4.0.0.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)

## Value

`BreakCornerBuilder.``Value`

  Returns the fillet radius or the setback value, depending on the type of the break corner.

  `-------------------------------------`

  Getter Method

  Signature `Value`

  Returns: | Either fillet radius or setback value (depending on the type of break corner)
  Return type: | `NXOpen.Expression`

  New in version NX4.0.0.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)

# Method Detail

## GetEdges

`BreakCornerBuilder.``GetEdges`

  The array of input edges for the break corner.

  Signature `GetEdges()`

  Returns: | Edge list
  Return type: | list of `NXOpen.Edge`

  New in version NX4.0.0.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)

## GetFaces

`BreakCornerBuilder.``GetFaces`

  The array of input faces that implicitly include all connected sharp thickness edges as input for the break corner.

  Signature `GetFaces()`

  Returns: | Face list
  Return type: | list of `NXOpen.Face`

  New in version NX4.0.0.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)

## SetEdges

`BreakCornerBuilder.``SetEdges`

  The array of input edges for the break corner.

  Signature `SetEdges(edges)`

  Parameters: | edges (list of `NXOpen.Edge`) – Edge list

  New in version NX4.0.0.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)

## SetFaces

`BreakCornerBuilder.``SetFaces`

  The array of input faces that implicitly include all connected sharp thickness edges as input for the break corner.

  Signature `SetFaces(faces)`

  Parameters: | faces (list of `NXOpen.Face`) – Face list

  New in version NX4.0.0.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)

## SetValue

`BreakCornerBuilder.``SetValue`

  Signature `SetValue(filletRadiusOrSetback)`

  Parameters: | filletRadiusOrSetback (str) – Either fillet radius or setback value (depending on the type of break corner)

  New in version NX4.0.0.

  Deprecated since version NX10.0.0: Use `Expression.RightHandSide()` on the `Expression` object returned from `Features.SheetMetal.BreakCornerBuilder.Value()` instead.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)

## Validate

`BreakCornerBuilder.``Validate`

  Validate whether the inputs to the component are sufficient for commit to be called.

  If the component is not in a state to commit then an exception is thrown. For example, if the component requires you to set some property, this method will throw an exception if you haven’t set it. This method throws a not-yet-implemented NXException for some components.

  Signature `Validate()`

  Returns: | Was self validation successful
  Return type: | bool

  New in version NX3.0.1.

  License requirements: None.

## ValidateBuilderData

`BreakCornerBuilder.``ValidateBuilderData`

  Verify that the builder data is valid for creating a break corner.

  If the Builder data is valid, return value is 0

  Signature `ValidateBuilderData()`

  Returns: | Data validity flag (zero for valid and non-zero for invalid)
  Return type: | int

  New in version NX4.0.0.

  License requirements: nx_sheet_metal (“NX Sheet Metal”) OR nx_flexible_pcb (“NX Flexible PCB”)