NXOpen.UF.Sf.UgsMeshAbstractionParams Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Sf.UgsMeshAbstractionParams Structure

NXOpen.UF.Sf.UgsMeshAbstractionParams is an alias for NXOpen.UF.SfUgsMeshAbstractionParams_Struct

class `NXOpen.UF.``SfUgsMeshAbstractionParams_Struct`

  Bases: `object`

  Refer to UF_SF_ugs_mesh_abstraction_params_s for documentation.

Fields

`NXOpen.UF.SfUgsMeshAbstractionParams_Struct.SmallFeature` | % of element length for abstraction
`NXOpen.UF.SfUgsMeshAbstractionParams_Struct.EdgeMergeToggle` | Edge merge toggle 0 or 1
`NXOpen.UF.SfUgsMeshAbstractionParams_Struct.EdgeAngle` | Edge merge angle
`NXOpen.UF.SfUgsMeshAbstractionParams_Struct.FilletToggle` | true => Filler detection ON false=> Fillet detection OFF
`NXOpen.UF.SfUgsMeshAbstractionParams_Struct.FilletType` | Used only if fillet_toggle == true Fillet type
`NXOpen.UF.SfUgsMeshAbstractionParams_Struct.FilletNumElem` | No of elements on a quarter arc of fillet
`NXOpen.UF.SfUgsMeshAbstractionParams_Struct.FilletMinRad` | Min radius
`NXOpen.UF.SfUgsMeshAbstractionParams_Struct.FilletMaxRad` | Max radius