RasterImageMaxTextureSize Enumeration — NXOpen Python API Reference 12.0.0 documentation

# RasterImageMaxTextureSize Enumeration

NXOpen.Features.RasterImage.MaxTextureSize is an alias for NXOpen.Features.RasterImageMaxTextureSize

class `NXOpen.Features.``RasterImageMaxTextureSize`

  Bases: `object`

  Specifies the maximum number of pixels to allow for the width or height of a raster image. If a size is requested which is larger than what the hardware can supported, the largest supported size will be used. All hardware can support at least 512x512 pixels.

  Enum Members

  Enum Member | Enum Member Description
  --- | ---
  N512 | 512 x 512 max size
  N1024 | 1024 x 1024 max size
  N2048 | 2048 x 2048 max size
  N4096 | 4096 x 4096 max size
  N8192 | 8192 x 8192 max size
  N16384 | 16384 x 16384 max size
  N32768 | 32768 x 32768 max size

  `ValueOf`()

    Returns enum member equivalent to the value passed. Useful for bit operations of enum members.

    Signature `ValueOf(value)`

    Parameters: | value – Any integer value or bit operation result of enum members:type value: int:returns: Enum member equivalent to the value passed.
    Return type: | Enum Member type.

    New in version NX9.0.1.

    License requirements: None.