InspectionLinear5axisMoveToPointBuilder Class — NXOpen Python API Reference 12.0.0 documentation

# InspectionLinear5axisMoveToPointBuilder Class

class `NXOpen.CAM.``InspectionLinear5axisMoveToPointBuilder`

  Bases: `NXOpen.CAM.InspectionMoveBuilder`

  Represents the builder for the CMM Inspection sub-operation Linear 5axis Move To Point.

  To create a new instance of this class, use `NXOpen.CAM.InspectionMoveCollection.CreateInspectionLinear5axisMoveToPointBuilder()`

  New in version NX8.5.0.

# Properties

Property | Description
--- | ---
AngleA | Returns or sets the A angle for an indexable head
AngleB | Returns or sets the B angle for an indexable head
ApproachDistance | Returns or sets the approach distance
DepthDistance | Returns or sets the depth distance
DepthMethod | Returns or sets the depth method
GotoAangle | Returns or sets the goto A angle
GotoBangle | Returns or sets the goto B angle
MotionType | Returns or sets the motion type
ProbeTipType | Returns or sets the preferred probe tip type
ProbeTipTypeBuilder | Returns the Probe Tip Type Builder
RetractDistance | Returns or sets the retract distance
SensorOpName | Returns or sets the inspection sensor operation name
SensorStrategy | Returns or sets the sensor selection strategy
SensorStrategyBuilder | Returns the Sensor Strategy Enum Builder
Tag | Returns the Tag for this object.
TargetPoint | Returns or sets the point
TipAngleMode | Returns or sets the tip angle selection mode
TipMode | Returns or sets the probe tip selection mode
TipNumber | Returns or sets the probe tip number

# Methods

Method | Description
--- | ---
Commit | Commits any edits that have been applied to the builder.
Destroy | Deletes the builder, and cleans up any objects created by the builder.
GetCommittedObjects | For builders that create more than one object, this method returns the objects that are created by commit.
GetObject | Returns the object currently being edited by this builder.
LockMove | Set lock to prevent move parameters from being changed programmatically.
SetParent | Set parent
SetProbeAngles | Set default values for probe angles based on feature type.
SetProbeTip | Set default probe tip based on preferred tip type and probe angles.
SetSibling | Set sibling
ShowResults | Updates the model to reflect the result of an edit to the model for all builders that support showing results.
Validate | Validate whether the inputs to the component are sufficient for commit to be called.

# Property Detail

## DepthDistance

`InspectionLinear5axisMoveToPointBuilder.``DepthDistance`

  Returns or sets the depth distance

  `-------------------------------------`

  Getter Method

  Signature `DepthDistance`

  Returns: |
  Return type: | float

  New in version NX9.0.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `DepthDistance`

  Parameters: | distance (float) –

  New in version NX9.0.0.

  License requirements: insp_programming (“INSPECTION PROGRAMMING”)

## DepthMethod

`InspectionLinear5axisMoveToPointBuilder.``DepthMethod`

  Returns or sets the depth method

  `-------------------------------------`

  Getter Method

  Signature `DepthMethod`

  Returns: |
  Return type: | `NXOpen.CAM.InspectionMoveBuilderDepthMethodTypes`

  New in version NX9.0.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `DepthMethod`

  Parameters: | method (`NXOpen.CAM.InspectionMoveBuilderDepthMethodTypes`) –

  New in version NX9.0.0.

  License requirements: insp_programming (“INSPECTION PROGRAMMING”)

## GotoAangle

`InspectionLinear5axisMoveToPointBuilder.``GotoAangle`

  Returns or sets the goto A angle

  `-------------------------------------`

  Getter Method

  Signature `GotoAangle`

  Returns: |
  Return type: | float

  New in version NX8.5.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `GotoAangle`

  Parameters: | gotoAangle (float) –

  New in version NX8.5.0.

  License requirements: insp_programming (“INSPECTION PROGRAMMING”)

## GotoBangle

`InspectionLinear5axisMoveToPointBuilder.``GotoBangle`

  Returns or sets the goto B angle

  `-------------------------------------`

  Getter Method

  Signature `GotoBangle`

  Returns: |
  Return type: | float

  New in version NX8.5.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `GotoBangle`

  Parameters: | gotoBangle (float) –

  New in version NX8.5.0.

  License requirements: insp_programming (“INSPECTION PROGRAMMING”)

## TargetPoint

`InspectionLinear5axisMoveToPointBuilder.``TargetPoint`

  Returns or sets the point

  `-------------------------------------`

  Getter Method

  Signature `TargetPoint`

  Returns: |
  Return type: | `NXOpen.Point`

  New in version NX8.5.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `TargetPoint`

  Parameters: | point (`NXOpen.Point`) –

  New in version NX8.5.0.

  License requirements: insp_programming (“INSPECTION PROGRAMMING”)

# Method Detail

## Validate

`InspectionLinear5axisMoveToPointBuilder.``Validate`

  Validate whether the inputs to the component are sufficient for commit to be called.

  If the component is not in a state to commit then an exception is thrown. For example, if the component requires you to set some property, this method will throw an exception if you haven’t set it. This method throws a not-yet-implemented NXException for some components.

  Signature `Validate()`

  Returns: | Was self validation successful
  Return type: | bool

  New in version NX3.0.1.

  License requirements: None.