BushingEADBuilder Class — NXOpen Python API Reference 12.0.0 documentation

# BushingEADBuilder Class

class `NXOpen.CAE.``BushingEADBuilder`

  Bases: `NXOpen.Builder`

  This class provides Bushing Associated Data Support

  To create a new instance of this class, use `NXOpen.CAE.NodeElementManager.CreateBushingEadBuilder()`

  New in version NX7.5.0.

# Properties

Property | Description
--- | ---
CsysDataType | Returns or sets the get selection csys data type gets coordinate system data type
Elements | Returns the select element operator selects elements
OriCsystem | Returns or sets the get coordinate system method gets the coordinate system for orienting by coordinate system
OriDirr | Returns or sets the get oriDirr operator gets orientaion vector value
OriMethod | Returns or sets the method to get the element orientation method
OriNode | Returns the get ori_node operator selects an orientation node
OrientationState | Returns or sets the state drives the commit action
PhysicalPropertyTable | Returns or sets the physical property table of the bushing element
PhysicalPropertyTableState | Returns or sets the physical property table state state drives the action upon commit
PointInPlane | Returns or sets the get coordinate system data point in plane gets the coordinates of point in x-z plane if cartesian csys or point in azimuthal origin plane if cylindrical/spherical csys for orientation
PointOnZaxis | Returns or sets the get coordinate system data point on z axis gets the coordinates of point on z-axis for orientation
PointOrigin | Returns or sets the get coordinate system data point origin gets the coordinates of origin point for orientation
PreferredLabel | Returns or sets the get preferred csys label gets the label assigned to the csys data
Tag | Returns the Tag for this object.

# Methods

Method | Description
--- | ---
Commit | Commits any edits that have been applied to the builder.
Destroy | Deletes the builder, and cleans up any objects created by the builder.
GetCommittedObjects | For builders that create more than one object, this method returns the objects that are created by commit.
GetObject | Returns the object currently being edited by this builder.
ShowResults | Updates the model to reflect the result of an edit to the model for all builders that support showing results.
Validate | Validate whether the inputs to the component are sufficient for commit to be called.

# Enumerations

BushingEADBuilderCoordinateSystemDataType Enumeration | indicates which type of coordinate system data to use
BushingEADBuilderOrientationMethod Enumeration | indicates which orientation method to use
BushingEADBuilderState Enumeration | indicates to ignore, apply or clear the state property upon commit

# Property Detail

## CsysDataType

`BushingEADBuilder.``CsysDataType`

  Returns or sets the get selection csys data type gets coordinate system data type

  `-------------------------------------`

  Getter Method

  Signature `CsysDataType`

  Returns: |
  Return type: | `NXOpen.CAE.BushingEADBuilderCoordinateSystemDataType`

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `CsysDataType`

  Parameters: | csysDataType (`NXOpen.CAE.BushingEADBuilderCoordinateSystemDataType`) –

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## Elements

`BushingEADBuilder.``Elements`

  Returns the select element operator selects elements

  `-------------------------------------`

  Getter Method

  Signature `Elements`

  Returns: |
  Return type: | `NXOpen.CAE.SelectElementsBuilder`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## OriCsystem

`BushingEADBuilder.``OriCsystem`

  Returns or sets the get coordinate system method gets the coordinate system for orienting by coordinate system

  `-------------------------------------`

  Getter Method

  Signature `OriCsystem`

  Returns: |
  Return type: | `NXOpen.CoordinateSystem`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `OriCsystem`

  Parameters: | oriCsystem (`NXOpen.CoordinateSystem`) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## OriDirr

`BushingEADBuilder.``OriDirr`

  Returns or sets the get oriDirr operator gets orientaion vector value

  `-------------------------------------`

  Getter Method

  Signature `OriDirr`

  Returns: |
  Return type: | `NXOpen.Direction`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `OriDirr`

  Parameters: | oriDirr (`NXOpen.Direction`) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## OriMethod

`BushingEADBuilder.``OriMethod`

  Returns or sets the method to get the element orientation method

  `-------------------------------------`

  Getter Method

  Signature `OriMethod`

  Returns: |
  Return type: | `NXOpen.CAE.BushingEADBuilderOrientationMethod`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `OriMethod`

  Parameters: | oriMethod (`NXOpen.CAE.BushingEADBuilderOrientationMethod`) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## OriNode

`BushingEADBuilder.``OriNode`

  Returns the get ori_node operator selects an orientation node

  `-------------------------------------`

  Getter Method

  Signature `OriNode`

  Returns: |
  Return type: | `NXOpen.CAE.SelectFENodeList`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## OrientationState

`BushingEADBuilder.``OrientationState`

  Returns or sets the state drives the commit action

  `-------------------------------------`

  Getter Method

  Signature `OrientationState`

  Returns: |
  Return type: | `NXOpen.CAE.BushingEADBuilderState`

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `OrientationState`

  Parameters: | orientationState (`NXOpen.CAE.BushingEADBuilderState`) –

  New in version NX7.5.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## PhysicalPropertyTable

`BushingEADBuilder.``PhysicalPropertyTable`

  Returns or sets the physical property table of the bushing element

  `-------------------------------------`

  Getter Method

  Signature `PhysicalPropertyTable`

  Returns: |
  Return type: | `NXOpen.CAE.PhysicalPropertyTable`

  New in version NX11.0.1.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `PhysicalPropertyTable`

  Parameters: | physicalPropertyTable (`NXOpen.CAE.PhysicalPropertyTable`) –

  New in version NX11.0.1.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## PhysicalPropertyTableState

`BushingEADBuilder.``PhysicalPropertyTableState`

  Returns or sets the physical property table state state drives the action upon commit

  `-------------------------------------`

  Getter Method

  Signature `PhysicalPropertyTableState`

  Returns: |
  Return type: | `NXOpen.CAE.BushingEADBuilderState`

  New in version NX11.0.1.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `PhysicalPropertyTableState`

  Parameters: | physicalPropertyTableState (`NXOpen.CAE.BushingEADBuilderState`) –

  New in version NX11.0.1.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## PointInPlane

`BushingEADBuilder.``PointInPlane`

  Returns or sets the get coordinate system data point in plane gets the coordinates of point in x-z plane if cartesian csys or point in azimuthal origin plane if cylindrical/spherical csys for orientation

  `-------------------------------------`

  Getter Method

  Signature `PointInPlane`

  Returns: | orientation csys data point in the x-z plane if cartesian csys or azimuthal origin plane if cylindrical/spherical csys
  Return type: | `NXOpen.Point`

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `PointInPlane`

  Parameters: | planePoint (`NXOpen.Point`) – orientation csys data point in the x-z plane if cartesian csys or azimuthal origin plane if cylindrical/spherical csys

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## PointOnZaxis

`BushingEADBuilder.``PointOnZaxis`

  Returns or sets the get coordinate system data point on z axis gets the coordinates of point on z-axis for orientation

  `-------------------------------------`

  Getter Method

  Signature `PointOnZaxis`

  Returns: | orientation csys data point on z-axis
  Return type: | `NXOpen.Point`

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `PointOnZaxis`

  Parameters: | zAxisPoint (`NXOpen.Point`) – orientation csys data point on z-axis

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## PointOrigin

`BushingEADBuilder.``PointOrigin`

  Returns or sets the get coordinate system data point origin gets the coordinates of origin point for orientation

  `-------------------------------------`

  Getter Method

  Signature `PointOrigin`

  Returns: | orientation csys data origin point
  Return type: | `NXOpen.Point`

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `PointOrigin`

  Parameters: | originPoint (`NXOpen.Point`) – orientation csys data origin point

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

## PreferredLabel

`BushingEADBuilder.``PreferredLabel`

  Returns or sets the get preferred csys label gets the label assigned to the csys data

  `-------------------------------------`

  Getter Method

  Signature `PreferredLabel`

  Returns: |
  Return type: | int

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

  `-------------------------------------`

  Setter Method

  Signature `PreferredLabel`

  Parameters: | preferredLabel (int) –

  New in version NX12.0.0.

  License requirements: nx_masterfem (“Finite Element Modeling”)

# Method Detail

## Validate

`BushingEADBuilder.``Validate`

  Validate whether the inputs to the component are sufficient for commit to be called.

  If the component is not in a state to commit then an exception is thrown. For example, if the component requires you to set some property, this method will throw an exception if you haven’t set it. This method throws a not-yet-implemented NXException for some components.

  Signature `Validate()`

  Returns: | Was self validation successful
  Return type: | bool

  New in version NX3.0.1.

  License requirements: None.