CoolingFittingData Class — NXOpen Python API Reference 12.0.0 documentation

# CoolingFittingData Class

class `NXOpen.Tooling.``CoolingFittingData`

  Bases: `NXOpen.TransientObject`

  Represents the cooling fitting data in Add Channel Fitting Builder.

  To create an instance of this object use `Tooling.ChannelFittingBuilder.CreateCoolingFittingData()`

  New in version NX7.5.0.

# Methods

Method | Description
--- | ---
AddFittingPoints | Add cooling fitting points to the fitting data.
ClearFittingPoints | Clear cooling fitting points from the fitting data.
Dispose | Dispose the part infomation to be cloned.

# Method Detail

## AddFittingPoints

`CoolingFittingData.``AddFittingPoints`

  Add cooling fitting points to the fitting data.

  Signature `AddFittingPoints(fittingPoint)`

  Parameters: | fittingPoint (`NXOpen.Point`) – the fitting point to be added.

  New in version NX7.5.0.

  License requirements: None.

## ClearFittingPoints

`CoolingFittingData.``ClearFittingPoints`

  Clear cooling fitting points from the fitting data.

  Signature `ClearFittingPoints()`

  New in version NX7.5.0.

  License requirements: None.

## Dispose

`CoolingFittingData.``Dispose`

  Dispose the part infomation to be cloned.

  Signature `Dispose()`

  New in version NX7.5.0.

  License requirements: None.