FeatureMillingCutParameters Class — NXOpen Python API Reference 12.0.0 documentation

# FeatureMillingCutParameters Class

class `NXOpen.CAM.``FeatureMillingCutParameters`

  Bases: `NXOpen.CAM.HoleMachiningCutParameters`

  Represents a FeatureMillingCutParameters Builder

  New in version NX9.0.2.

# Properties

Property | Description
--- | ---
BottomStock | Returns the bottom stock
CheckIpwCollisions | Returns or sets the value to Check for Ipw Collsions
CheckSafeClearance | Returns the Check Safe Clearance
CornerControl | Returns the corner control
CuttingDirection | Returns or sets the cut direction
HolderClearance | Returns the Holder Clearance
IpwType | Returns or sets the IPW type
NeckClearance | Returns the Neck Clearance
PartSafeClearance | Returns the Part Safe Clearance
PartStock | Returns the part stock
ShankClearance | Returns the Shank Clearance
Tag | Returns the Tag for this object.
Tolerances | Returns the Tolerances builder
TopOffset | Returns the top offset
UseToolHolder | Returns or sets the use tool holder

# Methods

# Enumerations

FeatureMillingCutParametersCuttingDirectionTypes Enumeration | cut direction options

# Property Detail

## CuttingDirection

`FeatureMillingCutParameters.``CuttingDirection`

  Returns or sets the cut direction

  `-------------------------------------`

  Getter Method

  Signature `CuttingDirection`

  Returns: | the cut directon type
  Return type: | `NXOpen.CAM.FeatureMillingCutParametersCuttingDirectionTypes`

  New in version NX9.0.2.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `CuttingDirection`

  Parameters: | cutDir (`NXOpen.CAM.FeatureMillingCutParametersCuttingDirectionTypes`) – the cut directon type

  New in version NX9.0.2.

  License requirements: cam_base (“CAM BASE”)