NXOpen.UF.Cutter.TurnTrackingPointData Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Cutter.TurnTrackingPointData Structure

NXOpen.UF.Cutter.TurnTrackingPointData is an alias for NXOpen.UF.CutterTurnTrackingPointData_Struct

class `NXOpen.UF.``CutterTurnTrackingPointData_Struct`

  Bases: `object`

  Refer to UF_CUTTER_turn_tracking_point_data_s for documentation.

Fields

`NXOpen.UF.CutterTurnTrackingPointData_Struct.Tlangl` | The tool angle of the point
`NXOpen.UF.CutterTurnTrackingPointData_Struct.Radius` | The radius value of the point
`NXOpen.UF.CutterTurnTrackingPointData_Struct.Xoff` | The postprocessor X offset of the point
`NXOpen.UF.CutterTurnTrackingPointData_Struct.Yoff` | The postprocessor Y offset of the point
`NXOpen.UF.CutterTurnTrackingPointData_Struct.Adjust` | The adjust register to use with this point
`NXOpen.UF.CutterTurnTrackingPointData_Struct.Cutcom` | The cutcom register to use with this point
`NXOpen.UF.CutterTurnTrackingPointData_Struct.Radiusid` | The radius id of this point
`NXOpen.UF.CutterTurnTrackingPointData_Struct.Cluster` | The P value of this point
`NXOpen.UF.CutterTurnTrackingPointData_Struct.Name` | The name of the tracking point