NXOpen.UF.Motion.Joint Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Motion.Joint Structure

NXOpen.UF.Motion.Joint is an alias for NXOpen.UF.MotionJoint_Struct

class `NXOpen.UF.``MotionJoint_Struct`

  Bases: `object`

  Refer to UF_MOTION_joint_s for documentation.

Fields

`NXOpen.UF.MotionJoint_Struct.Name` | The name of the joint.
`NXOpen.UF.MotionJoint_Struct.JtType` | The type of the joint.
`NXOpen.UF.MotionJoint_Struct.SnapLinks` | If TRUE, the joint “snaps” the two links into position using the link orientations.
`NXOpen.UF.MotionJoint_Struct.Link1` | The first link associated with the joint.
`NXOpen.UF.MotionJoint_Struct.Link2` | The second link associated with the joint.
`NXOpen.UF.MotionJoint_Struct.Direction1` | Smart direction tag that defines the direction of link_1.
`NXOpen.UF.MotionJoint_Struct.Direction2` | Smart direction tag that defines the direction of link_2.
`NXOpen.UF.MotionJoint_Struct.Origin1` | Optional point location on link_1.
`NXOpen.UF.MotionJoint_Struct.Origin2` | Optional point location on link_2.
`NXOpen.UF.MotionJoint_Struct.ScrewRatio` | Used only for UF_MOTION_screw_joint.