BendReportManagerMil98Report_Struct Struct — NXOpen Python API Reference 12.0.0 documentation

# BendReportManagerMil98Report_Struct Struct

NXOpen.Routing.BendReportManager.Mil98Report is an alias for NXOpen.Routing.BendReportManagerMil98Report_Struct

class `NXOpen.Routing.``BendReportManagerMil98Report_Struct`

  Bases: `object`

  Used in the MIL-D-9898 C specification reports.

  All values are absolute and cumulative. See MIL-D-9898C for more information. . Constructor: NXOpen.Routing.BendReportManager.Mil98Report()

# Fields

Field | Description
--- | ---
NXOpen.Routing.BendReportManagerMil98Report_Struct.C | The distance before the bend, from the start of the cable to the beginning point of the bend.
NXOpen.Routing.BendReportManagerMil98Report_Struct.F | The radius of the bend.
NXOpen.Routing.BendReportManagerMil98Report_Struct.E | The turn angle, this is the angle about the Y axis, relative to initial position (cumulation of the B value in YBC).
NXOpen.Routing.BendReportManagerMil98Report_Struct.G | The bend angle.
NXOpen.Routing.BendReportManagerMil98Report_Struct.Y | The Y value from the YBC format.

## C

`BendReportManagerMil98Report_Struct.``C`

  The distance before the bend, from the start of the cable to the beginning point of the bend.

  `-------------------------------------`

  Field Value Type:float

## F

`BendReportManagerMil98Report_Struct.``F`

  The radius of the bend.

  `-------------------------------------`

  Field Value Type:float

## E

`BendReportManagerMil98Report_Struct.``E`

  The turn angle, this is the angle about the Y axis, relative to initial position (cumulation of the B value in YBC).

  `-------------------------------------`

  Field Value Type:float

## G

`BendReportManagerMil98Report_Struct.``G`

  The bend angle.

  (The C value in YBC). `-------------------------------------`

  Field Value Type:float

## Y

`BendReportManagerMil98Report_Struct.``Y`

  The Y value from the YBC format.

  `-------------------------------------`

  Field Value Type:float