NXOpen.UF.Cutter.TrackingPointData Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Cutter.TrackingPointData Structure

NXOpen.UF.Cutter.TrackingPointData is an alias for NXOpen.UF.CutterTrackingPointData_Struct

class `NXOpen.UF.``CutterTrackingPointData_Struct`

  Bases: `object`

  Refer to UF_CUTTER_tracking_point_data_s for documentation.

Fields

`NXOpen.UF.CutterTrackingPointData_Struct.Diameter` | The output diameter of the point
`NXOpen.UF.CutterTrackingPointData_Struct.Distance` | The distance of the point along the tool axis
`NXOpen.UF.CutterTrackingPointData_Struct.Zoff` | The postprocessor Z offset of the point
`NXOpen.UF.CutterTrackingPointData_Struct.Adjust` | The adjust register to use with this point
`NXOpen.UF.CutterTrackingPointData_Struct.Cutcom` | The cutcom register to use with this point
`NXOpen.UF.CutterTrackingPointData_Struct.ZoffStatus` | The active/inactive status of the Z offset
`NXOpen.UF.CutterTrackingPointData_Struct.AdjustStatus` | The active/inactive status of the adjust register
`NXOpen.UF.CutterTrackingPointData_Struct.CutcomStatus` | The active/inactive status of the cutcom register
`NXOpen.UF.CutterTrackingPointData_Struct.Name` | The name of the tracking point