CurveFitOptions Class — NXOpen Python API Reference 12.0.0 documentation

# CurveFitOptions Class

class `NXOpen.GeometricUtilities.``CurveFitOptions`

  Bases: `NXOpen.TaggedObject`, `NXOpen.GeometricUtilities.IComponentBuilder`

  Represents the curve fit data

  New in version NX5.0.0.

# Properties

Property | Description
--- | ---
FitOption | Returns or sets the curve fit method
MaximumDegree | Returns or sets the maximum degree method
MaximumSegments | Returns or sets the maximum segments method
Tag | Returns the Tag for this object.

# Methods

Method | Description
--- | ---
Validate | Validate whether the inputs to the component are sufficient for commit to be called.

# Enumerations

CurveFitOptionsFitMethod Enumeration | Represents the curve fit method

# Property Detail

## FitOption

`CurveFitOptions.``FitOption`

  Returns or sets the curve fit method

  `-------------------------------------`

  Getter Method

  Signature `FitOption`

  Returns: | curve fit method
  Return type: | `NXOpen.GeometricUtilities.CurveFitOptionsFitMethod`

  New in version NX5.0.0.

  License requirements: solid_modeling (“SOLIDS MODELING”) OR cam_base (“CAM BASE”) OR geometric_tol (“GDT”) OR insp_programming (“INSPECTION PROGRAMMING”)

  `-------------------------------------`

  Setter Method

  Signature `FitOption`

  Parameters: | curveFitMethod (`NXOpen.GeometricUtilities.CurveFitOptionsFitMethod`) – curve fit method

  New in version NX5.0.0.

  License requirements: solid_modeling (“SOLIDS MODELING”) OR cam_base (“CAM BASE”) OR geometric_tol (“GDT”) OR insp_programming (“INSPECTION PROGRAMMING”)

## MaximumDegree

`CurveFitOptions.``MaximumDegree`

  Returns or sets the maximum degree method

  `-------------------------------------`

  Getter Method

  Signature `MaximumDegree`

  Returns: | maximum segments
  Return type: | int

  New in version NX5.0.0.

  License requirements: solid_modeling (“SOLIDS MODELING”) OR cam_base (“CAM BASE”) OR geometric_tol (“GDT”) OR insp_programming (“INSPECTION PROGRAMMING”)

  `-------------------------------------`

  Setter Method

  Signature `MaximumDegree`

  Parameters: | maximumDegree (int) – maximum degree method

  New in version NX5.0.0.

  License requirements: solid_modeling (“SOLIDS MODELING”) OR cam_base (“CAM BASE”) OR geometric_tol (“GDT”) OR insp_programming (“INSPECTION PROGRAMMING”)

## MaximumSegments

`CurveFitOptions.``MaximumSegments`

  Returns or sets the maximum segments method

  `-------------------------------------`

  Getter Method

  Signature `MaximumSegments`

  Returns: | maximum segments
  Return type: | int

  New in version NX5.0.0.

  License requirements: solid_modeling (“SOLIDS MODELING”) OR cam_base (“CAM BASE”) OR geometric_tol (“GDT”) OR insp_programming (“INSPECTION PROGRAMMING”)

  `-------------------------------------`

  Setter Method

  Signature `MaximumSegments`

  Parameters: | maximumSegments (int) – maximum segments

  New in version NX5.0.0.

  License requirements: solid_modeling (“SOLIDS MODELING”) OR cam_base (“CAM BASE”) OR geometric_tol (“GDT”) OR insp_programming (“INSPECTION PROGRAMMING”)

# Method Detail

## Validate

`CurveFitOptions.``Validate`

  Validate whether the inputs to the component are sufficient for commit to be called.

  If the component is not in a state to commit then an exception is thrown. For example, if the component requires you to set some property, this method will throw an exception if you haven’t set it. This method throws a not-yet-implemented NXException for some components.

  Signature `Validate()`

  Returns: | Was self validation successful
  Return type: | bool

  New in version NX3.0.1.

  License requirements: None.