NXOpen.UF.Motion.PointOnSurfaceData Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Motion.PointOnSurfaceData Structure

NXOpen.UF.Motion.PointOnSurfaceData is an alias for NXOpen.UF.MotionPointOnSurfaceData_Struct

class `NXOpen.UF.``MotionPointOnSurfaceData_Struct`

  Bases: `object`

  Refer to UF_MOTION_point_on_surface_data_s for documentation.

Fields

`NXOpen.UF.MotionPointOnSurfaceData_Struct.PointOnSurfaceTag` | Tag of the created/edited entity
`NXOpen.UF.MotionPointOnSurfaceData_Struct.PointTag` | The point tag of the point on surface constraint.
`NXOpen.UF.MotionPointOnSurfaceData_Struct.PointLinkTag` | Optional: The user need not specify this data.
`NXOpen.UF.MotionPointOnSurfaceData_Struct.NumFaceTags` | Number of face tags for the constraint
`NXOpen.UF.MotionPointOnSurfaceData_Struct.FaceTags` | Group of faces that can be have a parameterized UV space.
`NXOpen.UF.MotionPointOnSurfaceData_Struct.FaceLinkTag` | Optional: The user need not specify this data.
`NXOpen.UF.MotionPointOnSurfaceData_Struct.DisplayScale` | This scale is used in UI for displaying the object
`NXOpen.UF.MotionPointOnSurfaceData_Struct.EntityName` | A unique name for the object