NcmTransfer Class — NXOpen Python API Reference 12.0.0 documentation

# NcmTransfer Class

class `NXOpen.CAM.``NcmTransfer`

  Bases: `NXOpen.TaggedObject`

  Represents a `NXOpen.CAM.NcmTransfer`

  New in version NX9.0.0.

# Properties

Property | Description
--- | ---
ApplySafetyToDirect | Returns or sets the apply safety to direct value
MaxToolAxisChange | Returns or sets the max tool axis change
SafeDistanceBuilder | Returns the transfer between regions safe distance builder (inheritable tool dep)
Tag | Returns the Tag for this object.
Type | Returns or sets the transfer between levels type

# Methods

# Enumerations

NcmTransferTransferTypes Enumeration | Available types for transfer between regions in planar milling

# Property Detail

## ApplySafetyToDirect

`NcmTransfer.``ApplySafetyToDirect`

  Returns or sets the apply safety to direct value

  `-------------------------------------`

  Getter Method

  Signature `ApplySafetyToDirect`

  Returns: | the apply safety value
  Return type: | bool

  New in version NX9.0.3.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `ApplySafetyToDirect`

  Parameters: | applySafety (bool) – the apply safety value

  New in version NX9.0.3.

  License requirements: cam_base (“CAM BASE”)

## MaxToolAxisChange

`NcmTransfer.``MaxToolAxisChange`

  Returns or sets the max tool axis change

  `-------------------------------------`

  Getter Method

  Signature `MaxToolAxisChange`

  Returns: |
  Return type: | float

  New in version NX9.0.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `MaxToolAxisChange`

  Parameters: | newValue (float) –

  New in version NX9.0.0.

  License requirements: cam_base (“CAM BASE”)

## SafeDistanceBuilder

`NcmTransfer.``SafeDistanceBuilder`

  Returns the transfer between regions safe distance builder (inheritable tool dep)

  `-------------------------------------`

  Getter Method

  Signature `SafeDistanceBuilder`

  Returns: | The transfer between regions safe distance builder
  Return type: | `NXOpen.CAM.InheritableToolDepBuilder`

  New in version NX9.0.0.

  License requirements: None.

## Type

`NcmTransfer.``Type`

  Returns or sets the transfer between levels type

  `-------------------------------------`

  Getter Method

  Signature `Type`

  Returns: |
  Return type: | `NXOpen.CAM.NcmTransferTransferTypes`

  New in version NX9.0.0.

  License requirements: None.

  `-------------------------------------`

  Setter Method

  Signature `Type`

  Parameters: | transferType (`NXOpen.CAM.NcmTransferTransferTypes`) –

  New in version NX9.0.0.

  License requirements: cam_base (“CAM BASE”)