PartVisualizationShadeShadedViewToleranceType Enumeration — NXOpen Python API Reference 12.0.0 documentation

# PartVisualizationShadeShadedViewToleranceType Enumeration

NXOpen.Preferences.PartVisualizationShade.ShadedViewToleranceType is an alias for NXOpen.Preferences.PartVisualizationShadeShadedViewToleranceType

class `NXOpen.Preferences.``PartVisualizationShadeShadedViewToleranceType`

  Bases: `object`

  Describes the available tolerance types for Shaded View. Each of these options maps tolerance values to three specific faceting operations: Facet Edge Tolerance, Facet Chord Tolerance, and Angular Tolerance.

  Enum Members

  Enum Member | Enum Member Description
  --- | ---
  Coarse | For Coarse: Facet Edge Tolerance is 0.01, Facet Chord Tolerance is 0.01, and Angular Tolerance is 0.0
  Standard | For Standard: Facet Edge Tolerance is 0.005, Facet Chord Tolerance is 0.005 , and Angular Tolerance is 15
  Fine | For Fine: Facet Edge Tolerance is 0.0005, Facet Chord Tolerance is 0.0025, and Angular Tolerance is 6
  Extrafine | For Extrafine: Facet Edge Tolerance is 0.005, Facet Chord Tolerance is 0.001, and Angular Tolerance is 6
  Ultrafine | For Ultrafine: Facet Edge Tolerance is 0.0005, Facet Chord Tolerance is 0.0005, and Angular Tolerance is 3
  Customize | Customize. User can specify the Edge Tolerance, Face Tolerance and Angle Tolerance specifically.

  `ValueOf`()

    Returns enum member equivalent to the value passed. Useful for bit operations of enum members.

    Signature `ValueOf(value)`

    Parameters: | value – Any integer value or bit operation result of enum members:type value: int:returns: Enum member equivalent to the value passed.
    Return type: | Enum Member type.

    New in version NX9.0.1.

    License requirements: None.