CamProfileBuilderProfileCyclicType Enumeration — NXOpen Python API Reference 12.0.0 documentation

# CamProfileBuilderProfileCyclicType Enumeration

NXOpen.Mechatronics.CamProfileBuilder.ProfileCyclicType is an alias for NXOpen.Mechatronics.CamProfileBuilderProfileCyclicType

class `NXOpen.Mechatronics.``CamProfileBuilderProfileCyclicType`

  Bases: `object`

  Indicates which cyclic type should be take.The type of Cam Profile can be switched between non-cyclic, cyclic and relative cyclic

  Enum Members

  Enum Member | Enum Member Description
  --- | ---
  RelativeCyclic | In Relative Cyclic Cam Profiles the start point and end point of the profile do not necessarily have to be equal.
  Cyclic | In Cyclic Cam Profiles the points at the beginning and the end of the Master Axis range need to be identical with respect to Slave Axis value, slope and curve.
  NonCyclic | Non-cyclic Cam Profiles are defined only in the defined master axis range. Exceeding this range will cause an error.

  `ValueOf`()

    Returns enum member equivalent to the value passed. Useful for bit operations of enum members.

    Signature `ValueOf(value)`

    Parameters: | value – Any integer value or bit operation result of enum members:type value: int:returns: Enum member equivalent to the value passed.
    Return type: | Enum Member type.

    New in version NX9.0.1.

    License requirements: None.