NXOpen.UF.Sf.Ugs2dMeshParms Structure — NXOpen Python API Reference 12.0.0 documentation

# NXOpen.UF.Sf.Ugs2dMeshParms Structure

NXOpen.UF.Sf.Ugs2dMeshParms is an alias for NXOpen.UF.SfUgs2dMeshParms_Struct

class `NXOpen.UF.``SfUgs2dMeshParms_Struct`

  Bases: `object`

  Refer to UF_SF_ugs_2d_mesh_parms_s for documentation.

Fields

`NXOpen.UF.SfUgs2dMeshParms_Struct.ElementType` | Desired element type.
`NXOpen.UF.SfUgs2dMeshParms_Struct.ElementSize` | Desired element size.
`NXOpen.UF.SfUgs2dMeshParms_Struct.EdgeMatchToggle` | Edge merge toggle 0 or 1
`NXOpen.UF.SfUgs2dMeshParms_Struct.EdgeMatchTolerance` | edge matching tolerance.
`NXOpen.UF.SfUgs2dMeshParms_Struct.SuppressHoleToggle` | Suppress Hole toggle 0 or 1
`NXOpen.UF.SfUgs2dMeshParms_Struct.SuppressHoleDiameterValue` | Suppress Hole Diameter value.
`NXOpen.UF.SfUgs2dMeshParms_Struct.SuppressHolePointType` | 0- NONE, 1-POINT, 2-MESHPOINT
`NXOpen.UF.SfUgs2dMeshParms_Struct.TargetMinimumElementEdgeLength` | Target Minimum Element Edge Length toggle 0 or 1
`NXOpen.UF.SfUgs2dMeshParms_Struct.FormatMesh` | TRUE if 2d mesh is a shell mesh that should be formatted to the solver.
`NXOpen.UF.SfUgs2dMeshParms_Struct.AttemptQuadMapping` | TRUE if map mesher should be tried on faces for quad meshes or if free mesher should be called regardless of face shape.
`NXOpen.UF.SfUgs2dMeshParms_Struct.QuadOnlyOption` | Applies only when attempt_quad_mapping=FALSE Values are: 0 => Allow triangles OFF.
`NXOpen.UF.SfUgs2dMeshParms_Struct.SplitPoorQuads` | TRUE if poorly shaped quads should be split into triangles.
`NXOpen.UF.SfUgs2dMeshParms_Struct.MaximumQuadWarp` | if split_poor_quads == TRUE, this is the warp quality threshold. Any quad with greater warp than this will be split.
`NXOpen.UF.SfUgs2dMeshParms_Struct.MidnodeOption` | Whether to project midnodes or not.
`NXOpen.UF.SfUgs2dMeshParms_Struct.GeometryToleranceToggle` | Geometry Tolerance for midnode straightening
`NXOpen.UF.SfUgs2dMeshParms_Struct.GeometryToleranceValue` | Geometry Tolerance value for midnode straightening
`NXOpen.UF.SfUgs2dMeshParms_Struct.MaximumMidnodeJacobian` | If midnode_option = UF_SF_UGS_MESHER_mixed_midnodes, any element with a jacobian value higher than maximum_midnode_jacobian will have its midnodes straightened.
`NXOpen.UF.SfUgs2dMeshParms_Struct.MinimumFaceAngle` | Minimum angle at corner of a face that can support element.
`NXOpen.UF.SfUgs2dMeshParms_Struct.SurfMeshSizeVariation` | This controls how much variation in element size is desired/permitted in the mesh on the surface of the bodies being meshed.
`NXOpen.UF.SfUgs2dMeshParms_Struct.SmallFeature` | % of element length for abstraction
`NXOpen.UF.SfUgs2dMeshParms_Struct.EdgeMergeToggle` | Edge merge toggle 0 or 1
`NXOpen.UF.SfUgs2dMeshParms_Struct.EdgeAngle` | Edge merge angle
`NXOpen.UF.SfUgs2dMeshParms_Struct.MeshTransition` | Mesh transition 0=OFF,1=ON
`NXOpen.UF.SfUgs2dMeshParms_Struct.MultiBlockDecomposition` | Attempt MultiBlock Decomposition 0=OFF,1=ON
`NXOpen.UF.SfUgs2dMeshParms_Struct.MeshIndividualFaces` | Mesh Individual Faces 0=OFF,1=ON
`NXOpen.UF.SfUgs2dMeshParms_Struct.CadCurvatureAbstraction` | CAD Curvature Abstraction 0=OFF,1=ON
`NXOpen.UF.SfUgs2dMeshParms_Struct.MinimumFeatureLength` | Desired element size.
`NXOpen.UF.SfUgs2dMeshParms_Struct.MeshMethod` | 0 - Automatic, 1 - Paver
`NXOpen.UF.SfUgs2dMeshParms_Struct.FilletToggle` | true => Filler detection ON false=> Fillet detection OFF
`NXOpen.UF.SfUgs2dMeshParms_Struct.FilletType` | Used only if fillet_toggle == true Fillet type
`NXOpen.UF.SfUgs2dMeshParms_Struct.FilletNumElem` | No of elements on a quarter arc of fillet
`NXOpen.UF.SfUgs2dMeshParms_Struct.FilletMinRad` | Min radius
`NXOpen.UF.SfUgs2dMeshParms_Struct.FilletMaxRad` | Max radius
`NXOpen.UF.SfUgs2dMeshParms_Struct.MaxIncludedAngleQuadToggle` | Max Angle for quad Toggle state
`NXOpen.UF.SfUgs2dMeshParms_Struct.MinIncludedAngleQuadToggle` | Min Angle for quad Toggle state
`NXOpen.UF.SfUgs2dMeshParms_Struct.MaxIncludedAngleTriaToggle` | Max Angle for tria Toggle state
`NXOpen.UF.SfUgs2dMeshParms_Struct.MinIncludedAngleTriaToggle` | Min Angle for tria Toggle state
`NXOpen.UF.SfUgs2dMeshParms_Struct.MaxIncludedAngleQuadValue` | Max Angle for quad value
`NXOpen.UF.SfUgs2dMeshParms_Struct.MinIncludedAngleQuadValue` | Min Angle for quad value
`NXOpen.UF.SfUgs2dMeshParms_Struct.MaxIncludedAngleTriaValue` | Max Angle for tria value
`NXOpen.UF.SfUgs2dMeshParms_Struct.MinIncludedAngleTriaValue` | Min Angle for tria value
`NXOpen.UF.SfUgs2dMeshParms_Struct.MoveNodesOffGeometry` | Move Nodes Off Geometry
`NXOpen.UF.SfUgs2dMeshParms_Struct.MaxWarpToggle` |