LaminatePlyInterLaminarFailureTheoryType Enumeration — NXOpen Python API Reference 12.0.0 documentation

# LaminatePlyInterLaminarFailureTheoryType Enumeration

NXOpen.CAE.LaminatePly.InterLaminarFailureTheoryType is an alias for NXOpen.CAE.LaminatePlyInterLaminarFailureTheoryType

class `NXOpen.CAE.``LaminatePlyInterLaminarFailureTheoryType`

  Bases: `object`

  Inter-Laminar failure theory types

  Enum Members

  Enum Member | Enum Member Description
  --- | ---
  NotSet | No failure theory selected
  TransverseShearStress | Transverse Shear Stress inter-laminar failure criteria
  NormalStress | Normal Stress inter-laminar failure criteria
  UserDefined | User defined interlaminar failure theory (thru a user dll)

  `ValueOf`()

    Returns enum member equivalent to the value passed. Useful for bit operations of enum members.

    Signature `ValueOf(value)`

    Parameters: | value – Any integer value or bit operation result of enum members:type value: int:returns: Enum member equivalent to the value passed.
    Return type: | Enum Member type.

    New in version NX9.0.1.

    License requirements: None.